
	
	Guidance on the Installation and Use of Cross Pavement Charging Infrastructure

Permission to install cross pavement charging infrastructure to safely accommodate a cable to charge and electric vehicle from a residential premises is granted by the issue of a permit by Moray Council as the Roads Authority, through a Section 109 Agreement under the New Roads and Street Works Act 1991 (NRSWA).

A Section 109 Agreement allows a person or organisation to place, retain, inspect, maintain, adjust, repair, alter, or remove apparatus in a public road, and to carry out any works necessary for these purposes. A Section 109 Agreement also registers the infrastructure on the Scottish Road Works Commissioner’s system Scottish Community Apparatus Data Vault.

Subject to a successful application and conclusion of a Section 109 Agreement, the works must be undertaken by an approved, or suitably qualified, contractor Road Openings

Location
Not all locations are suitable for the installation of cross pavement charging infrastructure. The following criteria are considered by the Council when assessing the suitability of a location:

	
	Location/Property Type
	Permission Status
	Additional Notes/Requirements

	Off-Street Private Driveway
	Not applicable
	Off-street parking doesn’t require a cable gully.

	On-Street Public Footway (No Grass Verge)
	Potentially Suitable
	Pavement widths and parking demand would have to be factored into any decision, e.g. most suited to pavements at least 2 metres wide, and streets with low parking demand.

	On-Street Public Footway (with Grass Verge)
	Potentially suitable if service strip
	As well as the above considerations, grass verges may block installation due to lack of stability. If a grass verge is a service strip between a footway and carriageway, then it may be suitable.

	Public Road (No Footway)
	Not Permitted
	Cables cannot stretch over public roads without proper installation.

	Properties with Trees on Footway
	Potentially Suitable
	Tree roots and canopies interfere with safe installation.

	
	
	

	Location/Property Type
	Permission Status
	Additional Notes/Requirements

	On-Street Public Footway (with Parking Restrictions)
	Not Permitted, though opportunity for provision for Disabled Persons Parking Place
	Double yellow lines or other restrictions make installation ineligible.

	On-Street Parking (Restricted Parking Zone)
	Not Permitted
	Temporary restrictions may allow installation if accessible.

	Flats, Apartments, Tenements (No Private Space)
	Needs Permission
	Permission from building management required for installation (where the parking area is privately owned or managed). Parking demand would also have to be factored into any decision.

	Listed Buildings or Conservation Areas
	Needs Special Permission
	Additional planning permission required, subject to location rules.

	Parking Courts/Garage Blocks (Private Land)
	Not Allowed
	Not suitable for public gully installations, use private installations instead.

	Bus Stop or High Pedestrian Traffic Area
	Not Allowed
	High-traffic areas are not safe for cross- pavement installations. Local conditions assessment will be required.

	Roads not on the List of Public Roads but as a Council asset.
	Needs Special Permission
	Where the road/footway is a Council asset, permission from the relevant section, e.g. Housing, etc. will be required.

	Footways with lower kerb heights
	Potentially Suitable
	The base of the channel must be a minimum of 20mm above the level of the carriageway. As most channels are around 30mm in depth, this means that a minimum kerb height of 50mm must be present at the chosen location to enable the infrastructure.

	Footways where cross pavement charging infrastructure is already present
	Potentially Suitable
	There must be a minimum distance of 7.5 metres between each location where cross pavement charging infrastructure is present and proposed.











Type of Infrastructure
The Council will only support the use of specifically designed products for cross pavement charging infrastructure. The use of drainage or other infrastructure/products to accommodate cables will not be permitted. Details of the proposed Infrastructure, manufacturer and product number must be supplied as part of any application. In instances where 
Items/products are not specifically designed to accommodate charging cables, the Council will seek removal of the infrastructure. Any costs associated with the removal of the infrastructure will be met by the householder.
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Example of Acceptable Cross Pavement Infrastructure

Installation Requirements
Installation of the infrastructure must be undertaken by a Contractor who is on the Council’s list of contractors, or who is able to provide evidence of their public liability insurance and a current SWQR card and therefore approved to work on the Public Road. If the infrastructure is to be installed by the supplier of the infrastructure, then they will be required to provide all details necessary to become an approved contractor. Details of approved contractors can found at: Road Openings

Requirements for Approval
It is a condition of consent that applicants agree to the removal of the infrastructure when they sell or leave a property, unless otherwise agreed in writing with the Council and a new party who will be responsible for the maintenance of the infrastructure has been identified and has entered into an agreement with the Council. 



This is required as the infrastructure is registered on the Scottish Road Works Commissioner’s system Scottish Community Apparatus Data Vault, which is used by utilities companies, Councils and other contractors working on the public road. A named party responsible for the infrastructure must be provided on the system. Applicants must accept that they will burden the successor to the Title of the property with the conditions of any permission which may be granted and will subsequently record the conditions as part of that Title.


Conditions
1. IF YOU ARE APPLYING FOR GRANT FUNDING TO INSTALL THE INFRASTRUCTURE, PLEASE NOTE THAT CONSIDERATION OF THE SUITABILITY OF THE PROPOSED LOCATION CAN TAKE UP TO 3 WEEKS.

2. The proposed infrastructure must be specifically designed cross pavement charging product to accommodate a cable. The product must be ‘self-closing’ and must be flush with the level of the footway surface such that it does not present a trip hazard for pedestrians. The use of drainage infrastructure to accommodate a cable will not be permitted.

3. The proposed charging unit must not project into the public footway/road and must be contained within the property boundary. The storage of cables when not is use must also be within the property boundary and not project into the public footway/road. 

4. In Conservation Areas and at Listed Buildings, advice from the Council’s Development Management team must be sought: Do I Need Planning Permission?

5. The minimum width of unobstructed space between any boundary or building and the edge of the kerb must be no less than 1.5 metres, unless otherwise agreed with the Roads Authority. Note: Cross pavement cable infrastructure will not be permitted within the public carriageway.

6. The minimum height of the roadside kerb must be no less than 50mm.

7. Where cross pavement charging infrastructure is already present, there must be a minimum distance of 7.5 metres between existing and proposed infrastructure.

8. An approved, or suitably qualified, contractor must undertake the installation.

9. The applicant will be responsible for the maintenance of the infrastructure on and on-going basis and when requested by the Council, repair or replace the infrastructure and make good the surrounding footway. 

10. Unless otherwise agreed in writing with the Council, the infrastructure shall be removed and the surrounding footway made good, when the applicant sells/moves out of the property.

11. When using the infrastructure vehicles must be parked beside it. Charging cables must not be stretched across or along the public road, which includes the footway.

12. The presence of the infrastructure does not infer any right to park beside it. The public road beside the infrastructure will remain available for parking by all road users.

13. Applicants must agree to the removal of the cross pavement infrastructure at any time they are requested to do so by the Council, any Statutory Undertakers or by the emergency services.

14. Indemnity - The applicant shall indemnify Moray Council as Roads Authority for and against all actions, claims, demands, costs, charges, damages, losses and expenses of whatsoever kind or nature which may be brought or made against them or incurred by them in respect of the negligence, omission or default of the holder of this permission or those for whom the holder of this permission is responsible arising in respect of any operations authorised by this permission unless due to the negligence or other breach of legal duty on the part of the  Council or of any person for whom the Council are responsible.
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